During acquizition of Z-Stack do not touch computer keyboard or mouse.

It is assumed that the capture programs are installed as follows:

C:\Program Files\Canon\EOS Utility\EOS Utility.exe
C:\Program Files\Canon\RemoteCapture\RemoteCapture.exe
C:\Program Files\BreezeSys\DSLR Remote Pro\DSlrRemote.exe
C:\Program Files\HyperUtility\StudioUtility.exe

Capture program must not be running before clicking "Launch Capture Program" in ZStackTool.
If it was left open, close before starting ZStackTool.

If using Canon EOS Utility:

1. In Preferences check "Show [Camera settings/Remote shooting) Screen
2. Set Destination Folder and file Naming
3. The camera must be connected and active  (not sleeping). After clicking 
"Launch Capture Program" the camera control window must appear, not the main window.
If the main window appears, click on "Remote shooting".
4. Live View and Zoom View windows can be open but the camera control window
must be active (have focus) before you click on "Acquire Z-Stack" or 
"Capture single image" in the ZStackTool window.
5. Loading of EOS Utility takes time, be patient.

